# Background

Forensic firearms examiners analyze bullets through a process of visual feature comparison to determine whether two bullets originate from the same source. Two bullets in question are placed under a comparison microscope and firearms examiners evaluate similarities and differences between the bullets’ striation marks according to the AFTE Theory of Identification ([2](#_bookmark2)) guidelines resulting in a decision about whether both bullets were fired through the same gun barrel. In forensic science, this problem is known as the *same source- different source problem* and it focuses on establishing quantitative evidence whether two bullets were fired through the same gun barrel.

Recent advances in technology, particularly wider access to high resolution 3D microscopy tools, have led to an increase in research on image-analysis algorithms for auto- mated, quantitative analyses of bullet evidence. The introduction of such scanning technology to the field of forensic science allows for capture of high resolution 3D images of bullet LEAs, depicted in [Figure 1](#_bookmark14) (see [3](#_bookmark3); [4](#_bookmark4); [5](#_bookmark5)). The resulting 3D images have since been used in the development of several novel methods for automated comparison of land engraved areas (e.g. [6](#_bookmark6); [7](#_bookmark7); [8](#_bookmark8); [1](#_bookmark1)).

In this paper, we will focus only on barrels with traditional sharp-edged lands and grooves (i.e., no polygonal rifling). Sections of the bullet that make the closest contact with the barrel are called land engraved areas (LEAs). Those alternate with groove engraved areas (GEAs). Micro imperfections in the barrel introduce striae on the bullet during the firing process. The resulting striation marks provide evidence to address the same source- different source problem. A guiding principle in forensic firearms analysis is that two bullets fired through the same barrel will bear more similar striation marks on their LEAs than two bullets fired from different barrels. Hare et al. ([1](#_bookmark1)) proposes a matching algorithm based on 3D imaging data of LEAs. Horizontal slices of the 3D images, called crosscuts, provide a detailed representation of striae impressed on the surface at a horizontal cross- section of each LEA. A current limitation of this algorithm is that it cannot deal with a mix of striae from both LEA and GEAs. For the human visual system, separating the two areas is straightforward. However, the same cannot be said for automated computer vision techniques.

A correct identification of LEAs is vital to achieve high accuracy and precision in the subsequent downstream analysis and our goal is to present and discuss different automated methods for identifying so-called *shoulder locations*, the locations at which the land en- graved areas end and the groove engraved areas begin.

The structure of the paper is as follows: a description of the data storage format and data set, an explanation of methodology to predict shoulder locations, and finally an illustration of improved prediction accuracy results.

# Data Source

All currently published automated methods rely on high resolution 3D scans of bullet land engraved areas. Currently accepted best practice for collecting 3D images of bullet LEAs requires that bullets are staged such that striae appear vertically in the scan. Scanning across the LEA must begin and end in the neighboring groove engraved areas as shown in [Figure 2](#_bookmark15). Parts of the breakoff are captured as a visual reference for orientation (see [Figure 1](#_bookmark14)).

Scans are exported from the microscope as x3p files, conforming to the ISO5436-2 standard ([9](#_bookmark9)). Each scan is recorded as a matrix of prespecified (*x, y*) locations with a measured relative height value *z* for each (*x, y*) location on the LEA.

The algorithm proposed by Hare et al. ([1](#_bookmark1)) uses so-called crosscuts, height measurements along *x* for a fixed *y*. Removal of the overall curve of the bullet – the global structure captured in the 3D scanning process – transforms these crosscuts into to what Hare et al. ([1](#_bookmark1)) refer to as *signatures* (see [Figure 3](#_bookmark16)). The assessment of similarity between two LEAs is then based on a set of extracted features such as cross-correlation function, number of consecutively matching striae (see [10](#_bookmark10)) and maximum number of consecutively non-matching striae. Successful extraction of this set of features depends on how well we can remove the global bullet structure to translate from a crosscut to the corresponding signature.

In the following, we are introducing and comparing two methods for identifying shoulder locations. In order to assess the performance of these methods, we are applying both methods on 3D scans of LEAs from Hamby set 44 ([11](#_bookmark11)). Each Hamby set consists of 35 bullets fired from 10 consecutively rifled Ruger P85 barrels.

Each fired bullet in Hamby set 44 has 6 LEAs; every LEA was scanned for each of the 35 bullets, producing data for 210 individual lands. Two lands – Barrel 9, Bullet 2, Land 3 and Questioned Bullet L, Land 5 – were removed from consideration due to “tank rash”. Tank rash results from a bullet striking the bottom of a water recovery tank after exiting the barrel, thereby creating marks on the land that are not due to the contact with the barrel.

All 3D scans of Hamby Set 44 were captured at Iowa State University’s Roy J. Carver High Resolution Microscopy Facility with a Sensofar Confocal light microscope at 20 times magnification resulting in a resolution of 0.645 microns per pixel (1 micron = 1*µ*m = 0.001mm). Physically, each land is approximately 3 millimeters in width; as such, data structures for a single LEA can contain more than 3 million individual data points.

Data used to assess performance of the two methods consist of 2D crosscuts gathered from the 3D scans, as shown in Figure 4.

# Methodology

The structure in the 2D crosscuts is dominated by the curvature of the physical object (the bullet). To assess the similarity of features from two land engraved areas, this curvature has to be removed.

Non-parametric methods suggested in the literature, such as a LOESS fit ([1](#_bookmark1)) or a Gaussian filter ([7](#_bookmark7)) are effective for removing the curvature to extract a signature. However, they are prone to boundary effects, which cause mischaracterizations of data patterns near the boundaries of the data domain. In the case of crosscuts, the boundaries are often dominated by values originating from the GEA structure. This structure exaggerates existing boundary effects because GEAs introduce a secondary structure different from the main curvature of the LEA, as shown in [Figure 4](#_bookmark17) and [Figure 5](#_bookmark18). [Figure 4](#_bookmark17) shows how much a non-parametric LOESS fit is affected by including GEA data. [Figure 5](#_bookmark18) illustrates the effect the inclusion of the same has on extracted signatures. If included, GEA data result in strong boundary effects in the signatures. Statistically, GEA data introduce outliers into the LEA data. In the next sections, we introduce two methods for fitting the LEA structure. Both methods aim to describe the relationship between horizontal position and relative height on a crosscut. While the two approaches differ in methodology, they are both rooted in the ability to mitigate potential influence caused by outlying data.

In the following, we will describe the horizontal position on a crosscut of a scan as *xi* and measured relative height as *zi*, where *i* =1*,. . .,n*, the number of data points along a crosscut.

## *Robust Linear Models*

A natural candidate for a curved structure is a quadratic linear model of the form

where all error terms are considered independent and normally distributed with mean 0 and variance *σ*2. Parameter values of *, ,* are estimated by finding the values which minimize:

the vertical squared distance between each measured height value and the fitted curve. [Figure 6](#_bookmark19) shows that the presence of outliers near the boundaries pulls the resulting curve upwards towards groove engraved area data.

Alternatively, the curve can be fit by minimizing the absolute deviations in place of squared deviations:

This method of minimization is less influenced by large outliers present in the GEA data and the resulting model is known as a robust linear model.

Estimation based on taking squared deviations seeks to balance the fit between the LEA structure and the GEA structure, resulting in a fit which compromises between both structures without adequately fitting either. The use of absolute deviations reduces the degree of compromise in favor of fitting the majority structure, here LEA. Figure 6(a) and (c) show the fitted curves from each model framework. Figure 6(b) and (d) display the differences between predicted height and observed height at each location *xi*, known as the observed model residuals *ei*. We will utilize the observed residuals to separate the two structures. The robust model in Figure 6 fits the LEA structure more closely and better captures the curvature, allowing for a more accurate separation between GEA and LEA structures.

Because the robust approach results in residual values scattered near zero in the land engraved area and larger, mostly positive residuals in the groove engraved area, we will use high residual magnitude as an indicator of GEA membership (see [Figure 6](#_bookmark19)). High residual magnitude is determined using the median absolute deviation (MAD) of all residuals from a crosscut.

The MAD is a robust metric for the spread of data, similar to the standard deviation. It is preferable to the standard deviation to quantify the spread in situations with large outlying observations, such as the residuals in the groove engraved area.

Let *m* denote the median function. Then the MAD is defined as

Any residual value larger than 4*×*MAD is considered an outlier and likely a member of the GEA structure.

Shoulder location predictions are then calculated for each crosscut in the following manner (**Linear Shoulder Location Prediction**):

* 1. Fit a robust linear model of order 2 (i.e., quadratic) to the crosscut.
  2. Calculate a residual value *ei* for each data point on the crosscut.
  3. Calculate the residual median absolute deviation (MAD) for the crosscut.
  4. Remove all data points on the crosscut with a residual magnitude greater than 4*×*MAD.
  5. Identify the minimum *xL* and maximum *xR* of the remaining *xi* values. Then, *xL* and *xR* are the predicted left and right shoulder locations for that crosscut.

## *Robust LOESS*

One of the drawbacks of the linear approach is its rigidity in the shape of the curve. Locally weighted regression, known as LOESS, is a more flexible approach. This is advantageous when working with bullets, as it is unrealistic to expect a circular shape to remain after the bullet has been subjected to the forces of a gun barrel.

LOESS models estimate a predicted value *zi* for each height *zi* corresponding to location *xi* by estimating values *β*0*, β*1 which minimize

|  |  |  |
| --- | --- | --- |
|  |  | (1) |

where *wk*(*xi*) is a weight assigned to each data point *xk* based on its proximity to *xi.* Weights *wk* decrease as the distance to *xi* increases, so that data points closest to *xi* influence the prediction most. A LOESS model can also be described as a non-parametric weighted average of many parametric models fit to subsets of the data.

Although this approach allows for greater flexibility, LOESS models are affected more by GEA structures than robust linear models are. Data points near and in the GEA structure are most influenced by other GEA data rather than the overall global structure. This results in a set of predictions which misrepresents much of the data near the boundaries (see [Figure 7](#_bookmark20)).

Similar to the linear approach, there exists a robust approach to LOESS to adjust for these boundary effects.

The robust approach to LOESS uses an iterative re-weighting process to reduce the influence of outlying data points (see 12). First, an initial LOESS is fit. This step is followed by a redistribution of the weights *wk*(*xi*) based on residual values, . New weights are calculated as:

else, weights are set to 0. These new weights are re-applied in (1) and updated predictions are obtained. This reduces the influence of data points with large residual values *ek* in subsequent iterations. In the context of LEA crosscuts, the re-weighting reduces the influence of GEA data.

A robust LOESS model which accurately fits the LEA structure should result in a similar residual structure as that expected for the robust linear model: small residuals scattered near zero for *xi* locations in the land engraved area, and positive, possibly large residuals for *xi* locations in the groove engraved areas. The increased flexibility of LOESS models lead to a closer fit to the curvature and thus the robust LOESS more reliably results in the aforementioned residual pattern. We can thus use a lower cutoff for separation of the residuals via magnitude. A cutoff that performs well on the Hamby set 44 is twice the median absolute deviation (2 *× MAD*).

Shoulder location predictions are calculated for each crosscut in the following manner (LOESS shoulder location prediction):

* 1. Fit a robust LOESS model to the crosscut ([13](#_bookmark13)).
  2. Calculate a residual value *ei* for each data point on the crosscut.
  3. Calculate the residual median absolute deviation (MAD) for the crosscut.
  4. Remove all data points on the crosscut with a residual magnitude greater than 2*×*MAD.
  5. Identify the minimum *xL* and maximum *xR* of the remaining *xi* values. Then, *xL*

and *xR* are the predicted left and right shoulder locations for that crosscut.

One of the drawbacks of the linear approach is its rigidity in the shape of the curve. Locally weighted regression, known as LOESS, is a more flexible approach. This is advantageous when working with bullets, as it is unrealistic to expect a circular shape to remain after the bullet has been subjected to the forces of a gun barrel.

# Results

To quantitatively assess the predictive ability of the two alternative models, we first identified “ground truth” of shoulder locations by visual inspection for each of the 208 crosscuts in Hamby set 44.

As a performance measure, we define the error as the “area of misidentification”, i.e., the area of each crosscut which is identified incorrectly by the method. This metric is calculated for the left shoulder location as:

where is the set of points in crosscut *j* that fall between the predicted and actual left shoulder location, corresponds to the residual value at location from the robust LOESS fit to crosscut *j*, and is the distance between two subsequent locations in the crosscut. For the scans of Hamby set 44, this distance is equal to 0*.*645*µm* for all locations.

Similarly, the area is calculated for the right shoulder location as:

where is the set of points in crosscut *j* that fall between the predicted and actual right shoulder location.

Both the left and right areas of misidentification are thus in terms of microns2 and represent the area of loss we incur from incorrectly identifying a shoulder location.

Quantifying the results as an area is preferable to a distance metric as it captures not only the width of the profile area that is misidentified, but also the relative heights of the data. larger misidentified areas indicate larger portions of the GEA remain included in a profile, and thus signal an area which is more likely to have influence on an extracted signature. Smaller areas of misidentification suggest minimal loss in incurred, and these areas will have minimal effect on an extracted signature.

An area of misidentification was calculated separately for the left hand side and right hand side predictions for each of the 208 profiles in the data set, where predictions were based on the Robust Linear Model and Robust LOESS methods, as well as the Rollapply method suggested in Hare et al. (1).

To assess the performance of all three methods, we consider the distribution of the areas of misidentification across all 208 lands of Hamby set 44 (see Figure 8). A distribution starting at or close to zero with minimal spread is ideal as this suggests many of the predicted shoulder locations are very close to the manually identified locations, and predictions are removing many of the outlying GEA points. A distribution with a wider spread or many high, outlying areas of misidentification suggests a greater degree of uncertainty and inaccuracy for a particular method.

Because the raw distributions are difficult to visually compare due to extreme outliers, we categorized areas of misidentification as satisfactory, borderline, and unsatisfactory. Scores under 100 are considered satisfactory, scores between 100 and 1000 are borderline, and scores above 1000 are considered unsatisfactory (see [Figure 9](#_bookmark22)). Unsatisfactory cases are the most likely to cause poor or flawed results in subsequent analyses.

It is important to note that different results are expected for the left and right shoulder locations. Within Hamby set 44, almost all scans have a well-defined left groove. Left here is defined as visually left on the scan; this is the side the scan begins on, so a well-defined distinction between GEA and LEA is expected. Often, a less clear distinction is seen on the right side of the scan, with sometimes no apparent shoulder location visible. For this reason it is preferable to separate the left and right for visual inspection of results; a method may excel on one side but fall short on another.

# Conclusions

Both the robust linear model and robust LOESS approaches outperform currently implemented solutions based on data smoothers for the right shoulder location. Of the two, the robust LOESS approach clearly outperforms the robust linear model. This hierarchy of performance is well within expectation given the strength of robust approaches in general as well as the flexibility of LOESS applied to this data type. Robust LOESS also readily handles variation introduced in the process of translating the physical bullet into a 3D object. If there is too much variability in how the bullet is placed relative to the plane of reference on the microscope, profiles can have tilted shapes relative to the x-axis, which a quadratic linear model would fail to address. In these situations, LOESS excels.

While the proposed cutoff values as multiples of MAD work well on Hamby set 44, additional validation will need to be executed on a wider variety of barrel types. Depth of striae, physical size of bullet due to caliber, and non-traditional rifling techniques may require alterations to this cutoff value. In addition, a study of the effect of implementing robust LOESS shoulder location identification on the downstream similarity assessment will need to be completed. Due to increased accuracy of predicted shoulder locations, the authors expect an increase in accuracy in bullet matching algorithms. However, this will need to be validated on a variety of data sets prior to implementation without human intervention in the automated process.

# References

* 1. Hare E, Hofmann H, Carriquiry A. Automatic matching of bullet land impressions. The Annals of Applied Statistics 2017 12;11:2332–2356.
  2. AFTE Glossary. Theory of Identification as it Relates to Toolmarks. AFTE Journal 1998;30(1):86–88.
  3. De Kinder J, Prevot P, Pirlot M, Nys B. Surface topology of bullet striations: an innovating technique. AFTE Journal 1998;30(2):294–299.
  4. De Kinder J, Bonifanti M. Automated comparison of bullet striations based on 3D topography. Forensic Science International 1999;101:85–93.
  5. Bachrach B. Development of a 3D-based Automated Firearms Evidence Comparison System. Journal of Forensic Sciences 2002;47(6):1253–1264.
  6. Ma L, Song J, Whitenton E, Zheng A, Vorburger T, Zhou J. NIST bullet signature measurement system for RM (Reference Material) 8240 standard bullets. Journal of Forensic Sciences 2004;49(4):649–59.
  7. Chu W, Song T, Vorburger J, Yen J, Ballou S, Bacharach B. Pilot study of automated bullet signature identification based on topography measurements and correlations. Journal of Forensic Sciences 2010;55(2):341–47.
  8. Chu W, Thompson RM, Song J, Vorburger TV. Automatic identification of bullet signatures based on consecutive matching striae (CMS) criteria. Forensic Science International 2013;231(1-3):137–41.
  9. Geometrical product specifications (GPS) – Surface texture: Profile method; Measure- ment standards – Part 2: Software measurement standards. Geneva, CH: International Organization for Standardization; 2012.
  10. Biasotti AA. A Statistical Study of the Individual Characteristics of Fired Bullets. Journal of Forensic Sciences 1959;4(1):34–50.
  11. Hamby JE, Brundage DJ, Thorpe JW. The Identification of Bullets Fired from 10 Consecutively Rifled 9mm Ruger Pistol Barrels: A Research Project Involving 507 Participants from 20 Countries. AFTE Journal 2009;41(2):99–110.
  12. Cleveland WS. Robust Locally Weighted Regression and Smoothing Scatterplots. Journal of the American Statistical Association 1979;74(368):829–836.
  13. Loader C. locfit: Local Regression, Likelihood and Density Estimation.; 2013. R package version 1.5-9.1. [https://CRAN.R-project.org/package=locfit](https://CRAN.R-project.org/package%3Dlocfit).

# List of Tables

1. Table of results for areas of misidentification (in µ*m*2) resulting from automated shoulder location identification methods applied to Hamby set 44. Results are presented as percentage of shoulder location predictions which fall into each category: satisfactory (less than 100), borderline (between 100 and 1000), and unsatisfactory (greater than 1000).

**Left Shoulder Location Right Shoulder Location**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Method** | (0*,* 100) | (100*,* 1000) | (1000*, ∞*) | (0*,* 100) | (100*,* 1000) | (1000*, ∞*) |
| Rollapply | 86.54 | 8.17 | 5.29 | 52.88 | 34.13 | 12.98 |
| Robust Linear Model | 78.85 | 13.94 | 7.21 | 62.50 | 30.77 | 6.73 |
| Robust LOESS | 94.23 | 5.29 | 0.48 | 73.08 | 24.04 | 2.88 |

Table 1: Table of results for areas of misidentification (in *µm*2) resulting from automated shoulder location identification methods applied to Hamby set 44. Results are presented as percentage of shoulder location predictions which fall into each category: satisfactory (less than 100), borderline (between 100 and 1000), and unsatisfactory (greater than 1000).

# List of Figures

1. (Left) Close-up view of a bullet staged in a confocal light microscope. The green light marks the focal view of the capture area. (Right) Computer-rendered image of the scanned land engraved area with prominent striation marks. Breakoff is seen visually on the bottom right hand side on the scan.
2. Visualization of 3D data collected through high resolution scanning of a land engraved area. Striations on the surface of the object can be seen by viewing this data from “above”, as presented here.
3. The process of extracting a 2D signature from a 3D LEA scan described by (1). GEA removal between Steps 2 and 3 is critical to ensure precise signature extraction.
4. The black points show measured heights for a single crosscut of a 3D LEA scan. The main data structure, located in the center, is comprised of the land engraved area. The groove engraved areas are found on the left and right sides of the crosscut. The lines show fits of two non-parametric LOESS smooths, with and without GEA data. When GEA data is included, the smooth fails to estimate the main LEA structure near the boundaries.
5. An example of the impact failure to remove GEA data can have on an extracted 2D signature. Even though there are only very few points in the GEA structure, the extracted signatures are dominated by boundary effects.
6. Example of a quadratic linear model fit and resulting residuals (a, b) compared to a robust quadratic linear model fit and resulting residuals (c, d) for a single crosscut. The robust model is able to more effectively capture the curved structure of the LEA without begin influenced by the GEA. The dashed line in (d) is drawn at 4 x MAD. Values above the dashed line are considered outliers.
7. Example of a LOESS model fit and residuals (a, b) compared to a robust LOESS model fit and residuals (c, d) for a single profile. The robust model is again able to more effectively capture the curved structure of the LEA without being influenced by the GEA. The dashed line in (d) represents a cutoff of 2 x MAD. Values above the dashed line are considered outliers.
8. Distribution of areas of misidentification for rollapply (data smoothing) method, robust linear model method, and robust LOESS method, separated by left and right shoulder locations. A dense distribution with few high values indicates good performance across the LEAs in the data set.
9. Distribution of areas of misidentification for rollapply (data smoothing) method, robust linear model method, and robust LOESS method, separated by left and right shoulder locations. Areas of misidentification are placed into three categories: less than 100 microns squared (satisfactory), between 100 and 1000 microns squared (borderline), and greater than 1000 microns squared (unsatisfactory). A larger proportion of areas of misidentification under 100 microns squared indicates good performance across LEAs in the data set.